## Member Checklist for Interconnection

* Submit Net Metering Application
* Submit Interconnection Agreement
* Interconnection inverter must be UL 1741 Listed
* Electrical schematic drawing must be included
* Include provisions for a lockable visible disconnect.
* Send to: Tanner, PO Box 1426, North Bend, WA 98045-1426
* Receive written design approval from Tanner
* Get an electrical permit from Washington State L&I.
* Complete the installation.

Get inspections from a state electrical inspector and Tanner (call Tanner for inspection at 425-888-0623).

* If net metered, Tanner approves, or installs new, bi-directional meter.
* If production metered, Tanner installs a production meter after inspection approval.
* Submit Certificate of Completion to Tanner
* Start generating power

Questions?

Call the Tanner at 425-888-0623